CABQ Transportation HT#N08D006F Received 9/21/2020

Describe the future crossection of all streets in the study. Refer to the CABQ DPM TABLE 7.4.60 Street Element Dimensions, for City streets. Discuss any crossection that does not meet the latest DPM requirements. Include proposed bicycle facilities that are in the Bikeways and Trails Master Plan.

Amole is 30 MPH

Colobel use 30 MPH for the speed limit

Page 8, correct 1118th St to 118th St.

Auxiliary Lane Analysis table 43, refer to the CABQ DPM on City streets, *TABLE 7.4.68* **Turn Lane Warrants**. Use the NMDOT SAMM on Dennis Chavez.

Recommend including a traffic signal and intersection improvements in the infrastructure list at 98th and Amole Meas AV. Year 2027. Intersection spacing on 98th Gibson to Amole Mesa is favorable for a traffic signal 1/2-mile, Amole Mesa to Dennis Chavez is ¾ mile. The elementary school to the east would benefit from a traffic signal on 98th. There will be development to the east of 98th that would access this intersection.

Provide possible mitigation for the 118th St. Blvd. and Dennis Chavez Blvd.

Provide possible mitigation for the Condershire Dr.. and Dennis Chavez Blvd.